






77.75.101.166 is the ISP public ip.















The first one is the UTM to pfSense, second one is UTM to other UTM which works fine.



PFSense Phase1







PFSense Phase2

