

Interface eth0 was not used and i created the Hotspot\_1 there




Resulting in 3 interfaces




Made a copy of all the LAN firewall rules and replaced LAN with the Hotspot\_1 network







Added Hotspot\_1 to allowed networks for DNS




Created DHCP server range starting from 192.168.1.2 as the AP has 192.168.1.1




Reset my AP with DD-WRT firmware and reinstalled it the same as my other one used in my LAN




Disabled the firewall



Wireless Mode = AP




Wireless security disabled




Rebooted the AP, reconnected and rechecked settings before connecting it to the eth0 of Sophos UTM


From the 10.0.0.0/14 LAN I can ping the AP but cannot connect on the web GUI (perhaps needing a SNAT rule)




In UTM enabled the Hotspot



Hotspot log showing following



Added Hotspot\_1



After pressing Save immediately i received the password of the day.